For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Lower the headliner enough to gain access to the dome lamp housing--Refer to Headlining Trim Panel Replacement.

1 | Dome Lamp Lens
2 | Dome Lamp Switch Bezel
3 | Dome Lamp Housing Assembly

#### Procedure

1. Carefully use a flat-bladed tool, and release the tabs retaining the dome lamp to the headliner.
2. Disconnect the electrical connector.