For 1990-2009 cars

### Removal Procedure

Note: Do NOT disconnect engine coolant hoses.

1. Remove the radiator surge tank clip (2).
2. Remove the radiator surge tank (1)

Position the radiator surge tank (1) aside.

Note: Before disconnecting the reservoir tank hose, remove the clutch/brake fluid from the reservoir tank.

3. Remove the clutch master cylinder reservoir hose (1) from the reservoir tank and the master cylinder.

### Installation Procedure

1. Install the clutch master cylinder reservoir hose (1) to the reservoir tank and the master cylinder.
2. Fill the reservoir with clutch/brake fluid up to the MAX level.
3. Install the radiator surge tank (1).
4. Install the radiator surge tank clip (2).