For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove body side trim panel. Refer to Body Side Trim Panel Replacement - Right Side.
2. Disconnect battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.

1 | Radio Speaker Amplifier Disconnect electrical connectors.
2 | Radio Speaker Amplifier Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)