For 1990-2009 cars

#### Special Tools

• | EN 47519 Engine Bridge

• | EN 47650 Retainer Frame

• | EN 47650-030 Extension

• | EN 47650-050 Mounting Rail

• | EN 47650-250 Front Adapter

• | EN 47650-300 Rear Adapter

For equivalent regional tools refer to, Special Tools.

1. Remove the front fender shipping cover. Refer to Front Fender Shipping Cover Replacement.

Note: Do NOT tighten mounting nut (2) and adjustment screws (1).

2. Install EN 47650-300 adapter (3) to front compartment rail.

Note: Preset the EN 47650 frame off vehicle.

3. Preset EN 47650 frame

| Note: Outer bars of EN 47650 frame MUST be arranged parallel.

3.1. | Preset width (b) of EN 47650 frame

Specification
1425 mm (56 in)

3.2. | Preset distance (b) of EN 47650-250 adapters to outer bars of EN 47650 frame .

Specification
425 mm (17 in)

3.3. | Preset length (c) of EN 47650 frame

Specification
620 mm (25 in)

3.4. | Preset height (d) of EN 47650-250 adapters

Specification
140 mm (5.5 in)

3.5. | Tighten hexagons (1, 2) on both sides

4. With the aid of an assistant install EN 47650 frame (1) to the vehicle.
5. Tighten rear bolts of EN 47650 frame :

5.1. | Insert safety pins (2) through the EN 47650-250 adapters and the side bar to prevent movement.

5.2. | Tighten EN 47650 frame

to EN 47650-250 adapters with mounting bolts (1).

5.3. | Tighten mounting nuts (4) and of EN 47650-250 adapters .

5.4. | Tighten adjustment nuts (3, 5) of EN 47650-250 adapters .

6. Tighten front side of EN 47650 frame :

6.1. | Align the hook (2) with thumb wheel (3) to upper tie bar.

6.2. | Tighten the hook (2) to upper tie bar, using the thumb wheel (1).

7. Install EN 47650-050 rail (2) to EN 47650 frame .

Secure EN 7650-050 rail (2) with safety pins (3, 4).

Note: Secure chain boxes with hook chains on the outside of engine bride.

8. Install EN 47519 bridge with the aid of an assistant onto EN 7650-050 rail (2).

Secure EN 47519 bridge (5) with safety pins (3, 4).