For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Using a suitable jack stand, support the rear of the powertrain.
3. Remove the transmission bracket mount to mount through bolt (1).
4. Remove the transmission mount to transmission bolts (1).
5. Remove the transmission mount (2).

### Installation Procedure

1. Install the transmission mount (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the transmission mount to transmission bolts (1) and tighten to 100 N·m(74 lb ft).
3. Install the transmission bracket mount to mount through bolt (1) and tighten to 100 N·m(74 lb ft).
4. Remove the jack stand.
5. Lower the vehicle.