For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Position the window approximately half way down in the door.
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement.
3. Remove the outer sealing strip. Refer to Front Side Door Window Outer Sealing Strip Replacement.

1 | Front Side Door Window Regulator Sash Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)
2 | Front Side Door Window

#### Procedure

1. Loosen the window regulator sash nuts, pull upward to release the window from the sash.
2. Rotate the front door window as necessary to remove it from the door.