For 1990-2009 cars

Checks | Causes
--- | ---
Differential Assembly (232) |

• | Inspect for worn or damaged Side Gear Thrust Washer) or Pinion Gear Thrust Washer

• | Inspect for loose or worn Side Gear Axle Splines

• | Inspect for damaged or worn Side Gear

• | Inspect for worn or damaged Final Drive Inner and Outer Washers (584)

• | Inspect for loose, damaged or worn Front Differential Carrier Thrust Bearings, (228, 231, 233)

• | Inspect for broken, worn or disengaged Final Drive Pinion Pin Retainer (581)

• | Inspect for damaged or worn Pinion Gears

Drive Link Assembly (225) |

• | Inspect for worn, loose or damaged links

• | Inspect for broken, worn or loose Drive Link Lube Scoop (60)

Drive Sprocket Assembly (224) |

• | Inspect for improper Drive Sprocket (224) tooth surface finish

• | Inspect for broken or damaged Drive Sprocket (224) teeth

• | Inspect for worn or damaged Drive Sprocket Thrust Bearings (223, 556)

• | Inspect for worn or damaged Output Carrier Transfer Drive Gear Hub Assembly splines (222)

• | Inspect for loose, worn or damaged Output Carrier Transfer Drive Gear Hub Assembly bushing

Driven Sprocket Assembly (229) |

• | Inspect for worn, binding or damaged Driven Sprocket Bearing Assembly (228)

• | Inspect for worn or damaged Driven Sprocket Ball Bearing Assembly

• | Inspect for improper Driven Sprocket (229) tooth surface finish

• | Inspect for broken or damaged Driven Sprocket (229) teeth

Input Carrier Assembly (570) |

• | Inspect for pitted/spalled Pinion Gear teeth

• | Inspect for worn or damaged Pinion Gear Thrust Washers and Bushings

• | Inspect for worn or damaged Pinion Gears, Pins or Needle Bearings

• | Inspect for loose or broken Hub and Ring Gear

• | Inspect for loose or broken Output Internal Gear Retainer

• | Inspect for loose or worn Sun Gear Thrust Bearings (569, 572)

Output Carrier Assembly (574) |

• | Inspect for worn or damaged Pinion Gear Thrust Washers and Bushings

• | Inspect for worn or damaged Pinion Gears, Pins or Needle Bearings

• | Inspect for loose Hub and Ring Gear

Output Sun Gear Assembly (555) |

• | Inspect for worn or damaged Output Sun Gear Thrust Bearing (556)

• | Inspect for loose, worn or damaged Output Sun Gear bushing

• | Inspect for worn or damaged Output Sun Gear teeth

Reaction Carrier Assembly (567) |

• | Inspect for worn or damaged Pinion Gear Thrust Washers and Bushings

• | Inspect for worn or damaged Pinion Gears, Pins or Needle Bearings

• | Inspect for loose hub and Ring Gear

• | Inspect for worn or damaged Reaction Carrier Thrust Bearings (565)

Reaction Sun Gear Assembly (566) | Inspect for loose, worn or damaged Reaction Sun Gear Assembly bushing
Fluid Pump Assembly (201) |

1. Inspect for proper fluid level
2. Inspect for leaking Pump Fluid Outlet Seal Assembly (24) or Filter Seal

3-5-Reverse Clutch Assembly |

• | Inspect for inadequate Clutch Plate Clearance

• | Inspect for stripped or sheared Clutch Plate Splines (508-510)

• | Inspect for loose or worn Backing Plate Retainer (511)

• | Inspect for loose Speed Sensor Reluctor Wheel (501) or Retainer (500)

4-5-6 Clutch Assembly |

• | Inspect for inadequate Clutch Plate Clearance

• | Inspect for stripped or sheared Clutch Plate Splines (425-428)

• | Inspect for loose or worn Clutch Dam Retainer (524)

• | Inspect for loose or worn 3-5-Reverse/4-5-6 Clutch Housing Bushing

1-2-3-4 Clutch Assembly |

• | Inspect for inadequate Clutch Plate Clearance

• | Inspect for stripped or sheared Clutch Plate Splines (557-559)

• | Inspect for loose or worn Clutch Spring Retainer (561)

Low and Reverse Clutch Assembly (OWC) (543) |

• | Inspect for stripped or sheared Low and Reverse Clutch Assembly (543) splines

• | Inspect for non-rotating Low and Reverse Clutch Assembly (543)

Low and Reverse Clutch |

• | Inspect for inadequate Clutch Plate Clearance

• | Inspect for stripped or sheared Clutch Plate Splines (545-547)

• | Inspect for loose or worn Clutch Spring Retainer (548)

2-6 Clutch Assembly |

• | Inspect for inadequate Clutch Plate Clearance

• | Inspect for stripped or sheared Clutch Plate Splines (540-542)

• | Inspect for loose or worn Clutch Spring Retainer (537)

Case Assembly (50) |

• | Inspect for loose or broken Transmission Mount Bolts

• | Inspect for loose Torque Converter and Differential Housing Bolts (26)

• | Inspect for loose, worn or damaged differential bushing

• | Inspect for loose or broken Input Shaft Support Bolts (57)

• | Inspect for loose or broken Front Differential Carrier Baffle Bolts (61)

• | Inspect for stripped or sheared splines

• | Inspect for loose, worn or damaged bushing

Torque Converter Housing Assembly (208) |

• | Inspect for loose or broken Front Differential Ring Gear Retainer (206)

• | Inspect for loose, worn or damaged differential bushing

• | Inspect for loose or broken Pinion Gear Shaft Retainer Pin

• | Inspect for loose or broken Front Differential Carrier Baffle Bolts (204)

• | Inspect for loose or broken Fluid Pump Bolts (200)

• | Inspect for loose Torque Converter and Differential Housing Bolts (26)

• | Inspect for loose, worn or damaged bushing

Control Valve Body Cover Assembly (2) | Inspect for loose, missing or broken Valve Body Cover Bolts (1)
Torque Converter (28) |

• | Inspect for improper alignment of Torque Converter to the Crankshaft

• | Inspect for ballooning of the Torque Converter

Differential Carrier Assembly (232) |

• | Inspect for worn or damaged Differential Carrier (582)

• | Inspect for worn or damaged Pinion Pins (583)

• | Inspect for broken, worn or damaged Differential Sun Gear Bearing (231) or Driven Sprocket Bearing (228)

• | Inspect for worn or damaged Differential Side Gear teeth, Final Drive Pinion Gear (586) teeth or Final Drive Sun Gear (230) teeth

• | Inspect for worn or damaged Differential Side Gear Thrust Washers or Final Drive Inner and Outer Washers (584)

• | Inspect for worn or damaged Final Drive Rollers (585)

• | Inspect for broken or damaged Differential Pinion Gear Shaft Retainer