For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the body side trim panel. Refer to Body Side Trim Panel Replacement - Left Side.
2. Remove the rear window panel trim. Refer to Rear Window Panel Trim Replacement.

1 | Rear Seat Shoulder Belt Anchor Plate Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 45 N·m (33 lb ft)
2 | Rear Seat Shoulder Belt Retractor Bolt Tighten 45 N·m (33 lb ft)
3 | Rear Seat Shoulder Belt Assembly