For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the outside moisture cover. Refer to Windshield Outside Moisture Sensor Cover Replacement
2. Adjust the mirror to the full upward position.

1 | Inside Rearview Mirror Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (80 lb in)
2 | Inside Rearview Mirror Tip Slide the mirror in an upward motion in order to remove.