For 1990-2009 cars

### Removal Procedure

1. Open the hood.

Note: If the engine oil level is at maximum, some oil may emerge when drawing out the oil dipstick guide tube.

2. Place collecting basin underneath.
3. Remove the oil level indicator tube bolt (1).
4. Remove the oil level indicator tube (2).

### Installation Procedure

1. Install the oil level indicator tube (2).

Use a NEW oil level indicator tube gasket.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the oil level indicator tube bolt (1) and tighten to 8 N·m (71 lb in).
3. Close the hood.