For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

It is only necessary to lower the headliner. Only perform the steps in the headliner replacement procedure that will lower the headliner enough to gain access to the part. Refer to Headlining Trim Panel Replacement.

1 | Sunroof Window Motor Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 4 N·m (36 lb in)
2 | Sunroof Window Motor Assembly Tip Disconnect the electrical connector.