For 1990-2009 cars

## Clutch Actuator Cylinder Front Pipe Replacement D16

### Removal Procedure

1. Remove the battery tray. Refer to Battery Tray Replacement.

Note: Do NOT disconnect engine coolant hoses.

2. Remove the radiator surge tank clip (2).
3. Remove the radiator surge tank (1).

Position the radiator surge tank (1) aside.

Note: Before disconnecting the clutch actuator cylinder front pipe, remove the clutch/brake fluid from the reservoir tank.

4. Remove the clutch actuator cylinder front pipe retainer (1, 4).
5. Remove the clutch actuator cylinder front pipe from the retainer (3).
6. Remove the clutch actuator cylinder front pipe (2).

### Installation Procedure

1. Install the clutch actuator cylinder front pipe (2).
2. Install the clutch actuator cylinder front pipe to the retainer (3).
3. Install the clutch actuator cylinder front pipe retainer (1, 4).
4. Bleed the hydraulic clutch system. Refer to Hydraulic Clutch Bleeding.
5. Fill the reservoir with clutch/brake fluid up to the MAX level.
6. Install the radiator surge tank (1)
7. Install the radiator surge tank clip (2).
8. Install the battery tray. Refer to Battery Tray Replacement.

## Clutch Actuator Cylinder Front Pipe Replacement D33

### Removal Procedure

1. Remove the battery tray. Refer to Battery Tray Replacement.

Note: Do NOT disconnect engine coolant hoses.

2. Remove the radiator surge tank clip (2).
3. Remove the radiator surge tank (1).

Position the radiator surge tank (1) aside.

Note: Before disconnecting the clutch actuator cylinder front pipe, remove the clutch/brake fluid from the reservoir tank.

4. Remove the clutch actuator cylinder front pipe retainer (1, 4).
5. Remove the clutch actuator cylinder front pipe from the retainer (3).
6. Remove the clutch actuator cylinder front pipe (2).

### Installation Procedure

1. Install the clutch actuator cylinder front pipe (2).
2. Install the clutch actuator cylinder front pipe to the retainer (3).
3. Install the clutch actuator cylinder front pipe retainer (1, 4).
4. Bleed the hydraulic clutch system. Refer to Hydraulic Clutch Bleeding.
5. Fill the reservoir with clutch/brake fluid up to the MAX level.
6. Install the radiator surge tank (1).
7. Install the radiator surge tank clip (2).
8. Install the battery tray. Refer to Battery Tray Replacement.