For 1990-2009 cars

#### Special Tools

• | GE-39400-A Halogen Leak Detector

• | GE-46246 Valve Core Removal Tool

For equivalent regional tools, refer to Special Tools.

### Removal Procedure

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the service port valve core (1) using GE-46246 remover .

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the service port valve core using (1) GE-46246 remover and tighten to 3 N·m (22 lb in).
2. Evacuate and charge the refrigerant system. Refer to Refrigerant Recovery and Recharging.
3. Leak test the fittings using the GE-39400-A detector .