For 1990-2009 cars

Caution: Refer to Fastener Caution in the Preface section.

1. Install the 4 glow plugs (1) and tighten to 9 N·m (80 lb in) .
2. Install the 4 glow plug wiring harness plugs (1).
3. Install the glow plug heat shield (1).
4. Install the engine lift bracket nut (2) and tighten to 28 N·m (21 lb ft) .
5. Install the 3 glow plug heat shield bolts (3) and tighten to 20 N·m (15 lb ft) .