For 1990-2009 cars

1. Install the intake air pressure and temperature sensor gasket (4).
2. Install the intake air pressure and temperature sensor (2).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the intake air pressure and temperature sensor bolt (3) and tighten to 8 N·m (71 lb in) .
4. Install the coolant temperature sensor (1) and tighten to XXXN·m (XXX lb ft) .
5. Install the thermostat (2) to the intake manifold (1).
6. Install the thermostat housing gasket (5).
7. Install the thermostat housing (3).
8. Install the 2 thermostat housing bolts (4) and tighten to 23 N·m (17 lb in) .