For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the lower control arm. Refer to Lower Control Arm Replacement.

1 | Lower Control Arm Rear Bushing Bolt Tip Note the position of the bushing during removal.
2 | Lower Control Arm Rear Bushing Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Hold the rear bushing inner sleeve when tightening the rear bushing bolt.

Tighten
xx N·m (xx lb ft)