For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle
2. Disconnect the forward lamp electrical harness connector from the fog lamp bulb socket.

1 | Front Fog Lamp Projector Bulb Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

Rotate the bulb socket counterclockwise to remove from the lamp housing.

2 | Front Fog Lamp Assembly

#### Procedure

Remove the lamp assembly from the fog lamp bracket.