For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove instrument panel lower cluster trim plate. Refer to Instrument Panel Cluster Lower Trim Plate Replacement.
2. Remove instrument panel steering column upper trim cover. Refer to Steering Column Upper Trim Cover Replacement.

1 | Instrument Cluster Screw (2) (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Instrument Cluster Assembly