For 1990-2009 cars

callout | Component Name
--- | ---
1 | Bolt Access Plug

#### Procedure

Use a plastic flat-bladed tool to remove.

2 | Front Side Door Outside Handle Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten xx N·m(xx lb ft)
3 | Front Side Door Lock Cylinder

#### Procedure

1. Pull the lock cylinder from the housing to remove.
2. Inspect the lock, lock cylinder and handle adjustments. Refer to Front Side Door Outside Handle Rod Adjustment.

Tip
Pull the front side door outside handle to unlock the door lock cylinder.