For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Gasoline/Gasoline Vapors Warning in the Preface section.

#### Preliminary Procedure

1. Disconnect the battery negative cable Battery Negative Cable Disconnection and Connection.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Fuel Filter Cap Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (19 lb in)
2 | Fuel Filter Sealant
3 | Fuel Filter