For 1990-2009 cars

#### Special Tools

EN 6009 Remover and Installer Ignition Coil

For equivalent regional tools, refer to Special Tools.

### Removal Procedure

1. Remove the engine wiring harness guide (1) from the cylinder head.
2. Disconnect the ignition coil plug (2).

Note: Note the arrow on the cover.

3. Remove the cover of the ignition coil in the direction of the arrow.
4. Remove the 2 ignition coil bolts.
5. Install the EN 6009 remover/installer (1).
6. Remove the ignition coil (2).
7. Remove the EN 6009 remover/installer (1).

### Installation Procedure

Note: When installing a new ignition coil it is not necessary to replace the gaskets.

1. Install the EN 6009 remover/installer .
2. Install the ignition coil (1) and the NEW gaskets (2).

Caution: Refer to Fastener Caution in the Preface section.

Note: Note the arrow on the cover.

3. Install the 2 ignition coil bolts an tighten to 8 N·m (71 lb in).
4. Install the ignition coil cover in the direction of the arrow.
5. Connect the ignition coil plug (2).
6. Install the engine wiring harness guide (1) at the cylinder head.