For 1990-2009 cars

1. Inspect the water pump.

Note:

• | Ensure that the engine block surface and water pump surface are clear of old gasket material.

• | Do not immerse the water pump in solvent. The solvent may enter the water pump's permanently lubricated bearings and cause premature bearing failure.

2. Rotate the water pump drive pulley.

Note: The water pump drive pulley and impeller should turn straight and smoothly. If the drive pulley wobbles, is noisy, or feels rough when rotating, replace the water pump.

3. Install a NEW water pump gasket. (2).
4. Install the water pump (1).

Caution: Refer to Fastener Caution in the Preface section.

5. Install the 5 water pump bolts (3) and tighten to 11 N·m (97 lb in) .