For 1990-2009 cars

### Removal Procedure

Warning: Refer to Approved Equipment for Collision Repair Warning in the Preface section.

Warning: Refer to Collision Sectioning Warning in the Preface section.

Warning: Refer to Glass and Sheet Metal Handling Warning in the Preface section.

1. Disable the SIR System. Refer to SIR Disabling and Enabling.
2. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
3. Remove all related panels and components.
4. Visually inspect the damage. Repair as much of the damage as possible.
5. Remove the sealers and anti-corrosion materials from the repair area, as necessary. Refer to Anti-Corrosion Treatment and Repair.
6. Locate and mark all the necessary factory welds of the body side outer panel reinforcement.
7. Drill all factory welds. Note the number and location of welds for installation of the service assembly.
8. Remove the damaged body side outer panel reinforcement.

### Installation Procedure

1. Align the body side outer panel reinforcement.
2. Drill 8 mm (5/16 in) for plug welding along the edges of the body side outer panel reinforcement as noted from the original panel.
3. Clean and prepare the attaching surfaces for welding.
4. Position the body side outer panel reinforcement on the vehicle.
5. Verify the fit of thebody side outer panel reinforcement.
6. Clamp the body side outer panel reinforcement into position.
7. Plug weld accordingly.
8. Apply the sealers and anti-corrosion materials to the repair area, as necessary. Refer to Anti-Corrosion Treatment and Repair.
9. Paint the repaired area. Refer to Basecoat/Clearcoat Paint Systems.
10. Install all related panels and components.
11. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
12. Enable the SIR system. Refer to SIR Disabling and Enabling.