For 1990-2009 cars

Warning: Refer to Brake Dust Warning in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
3. Remove the brake drum. Refer to Brake Drum Replacement.
4. Turn in adjustment assembly (1) as far as possible.
5. Install brake drum. Refer to Brake Drum Replacement.
6. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation
7. Lower vehicle.
8. Apply the brake pedal at least 10 times. Verify the clicking sound of the adjuster assembly is not audible from either brake drum.
9. Adjust the park brake. Refer to Parking Brake Adjustment.