For 1990-2009 cars

### Removal Procedure

1. Remove instrument outer trim cover - left side. Refer to Instrument Panel Outer Trim Cover Replacement - Left Side.
2. Remove instrument panel lower trim pad cover - left side. Refer to Instrument Panel Lower Trim Pad Cover Replacement.
3. Remove floor air outlet duct (1) - left side.

### Installation Procedure

1. Install floor air outlet duct (1) - left side.
2. Install instrument panel lower trim pad cover - left side. Refer to Instrument Panel Lower Trim Pad Cover Replacement.
3. Install instrument outer trim cover - left side. Refer to Instrument Panel Outer Trim Cover Replacement - Left Side.