For 1990-2009 cars

| Note: Squeaks and rattles are caused by improperly controlled relative motion between vehicle components. There are 4 ways to prevent squeaks and rattles.

• | Attach the component that squeaks or rattles securely.

• | Separate the components that squeak or rattle to prevent contact.

• | Insulate the components that squeak or rattle.

• | Insulate low uniform friction surfaces to eliminate stickslip motion.