For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Radiator Grille Reinforcement Support Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in).
2 | Radiator Grille Reinforcement Support Retainer (Qty: 3)
3 | Radiator Grille Reinforcement Support