For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you review the General Description and perform the necessary inspections? | -- | Go to | Go to Symptoms - Suspension General Diagnosis
2 | Road test the vehicle in order to verify the customer's complaint. Does the vehicle operate normally? | -- | System OK | Go to
3 |

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Inspect for tire or wheel damage.

Did you find and correct the condition?

--

Go to

Go to

4 | Road test the vehicle to verify the location of the wheel bearing noise, preferably by using the CH 39570 Chassis Ear or equivalent. Did you locate the source of the wheel bearing noise? | -- | Go to | Go to
5 |

Note: Support the vehicle by the lower control arms or the rear axle to prevent movement during wheel bearing/hub inspection.

2. Mount and secure the GE-572 Dial Indicator or equivalent.
3. Ensure that the dial indicator contacts the vertical surface of the wheel as close as possible to the top wheel stud.
4. Push and pull on the top of the tire in order to inspect the total travel indicated by the dial indicator.

Is the measurement greater then the specified value?

0.127 mm (0.005 in)

Go to

System OK

6 | Replace the wheel bearing. Refer to Front Wheel Bearing and Hub Replacement or Rear Wheel Bearing and Hub Replacement. Did you complete the repair? | -- | Go to | --
7 | Road test the vehicle to verify the repair. Does the vehicle operate normally? | -- | System OK | Go to