For 1990-2009 cars

#### Special Tools

EN-45059 Torque Angle Sensor Kit

For equivalent regional tools, refer to Special Tools.

1. Install the piston and connecting rod assembly (4).
2. Install the connecting rod bearing (3).
3. Install the connecting rod cap (1).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the connecting rod bolts (2) and tighten to 35 N·m (26 lb ft) + 45 degrees use the EN-45059 sensor kit .
5. Assemble the caps and connecting rods in the marked position.
6. Rotate the crankshaft to a position where the connecting rod bolts are in the best situation for install.