For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the air cleaner housing. Refer to Air Cleaner Assembly Replacement.
2. Support the engine. Refer to Engine/Transmission Mounting.

1 | Engine Mount Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 58 N·m (43 lb ft)
2 | Engine Mount Bolt (Qty: 2) Tighten 62 N·m (46 lb ft)
3 | Engine Mount Bracket Bolt (Qty: 3) Tighten 55 N·m (41 lb ft)
4 | Engine Mount