For 1990-2009 cars

## Fastener Tightening Specifications 2.0L Diesel LLW

Application | Specification
--- | ---
Metric | English
Catalytic Converter Bracket Bolt | 40 N·m | 30 lb ft
Catalytic Converter Clamp | 40 N·m | 30 lb ft
Catalytic Converter Heat Shield Bolt | 20 N·m | 15 lb ft
Catalytic Converter Heat Shield Nut | 20 N·m | 15 lb ft
Engine Lift Bracket Nut | 28 N·m | 21 lb ft
Exhaust Flex Pipe to Exhaust Particulate Filter Nut | 40 N·m | 30 lb ft
Exhaust Front Hanger Bracket Nut | 20 N·m | 15 lb ft
Exhaust Front Pipe-to-Underbody Shield Nut | 2.5 N·m | 23 lb in
Exhaust Front/Rear Muffler Shield Nut | 2.5 N·m | 23 lb in
Exhaust Manifold Heat Shield Bolt | 20 N·m | 15 lb ft
Exhaust Manifold Nut | 33 N·m | 25 lb ft
Exhaust Particulate Filter Hanger Bracket Bolt | 17 N·m | 13 lb ft
Exhaust Pipe Clamp | XX | XX
Exhaust Temperature Sensor 1 | 45 N·m | 33 lb ft
Exhaust Temperature Sensor 2 | 45 N·m | 33 lb ft
PCV Valve Nut | 11 N·m | 98 lb in