For 1990-2009 cars

Caution:

• | Use care when servicing the fuel system components, especially the fuel injector electrical connectors, the fuel injector tips, and the injector O-rings. Plug the inlet and the outlet ports of the fuel rail in order to prevent contamination.

• | Do not use compressed air to clean the fuel rail assembly as this may damage the fuel rail components.

• | Do not immerse the fuel rail assembly in a solvent bath in order to prevent damage to the fuel rail assembly.

1. Install 4 NEW fuel injector gaskets (2).
2. Install the 4 injectors.
3. Shift the fuel injector bracket (2) and the bolt (1) with the washer (3) forward.

Caution: Refer to Fastener Caution in the Preface section.

4. Tighten the fuel injector bracket bolt to 28 N·m (21 lb ft).

Note: Inspect the gaskets before installation, replace if damaged.

5. Install the hole plugs and the hole plug gaskets (2, 3).
6. Install the hole plug bolts (1) and tighten to 7 N·m (62 lb in).