For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Gasoline/Gasoline Vapors Warning in the Preface section.

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Install a suitable hose at the fuel filter water bleed screw.

1 | Fuel Filter Water Bleed Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (23 lb in)