For 1990-2009 cars

An automobile engine is a combination of many of the following surfaces:

• | Machined

• | Honed

• | Polished

• | Lapped

The tolerances of these surfaces are measured in the ten-thousandths of an inch. When you service any internal engine part, cleanliness and care are important. Apply a liberal coating of engine oil to the friction areas during assembly in order to protect and lubricate the surfaces on initial operation. Throughout this section, practice proper cleaning and protection procedures to the machined surfaces and to the friction areas.

Caution: Engine damage may result if an abrasive paper, pad, or motorized wire brush is used to clean any engine gasket surfaces.

Whenever you remove the valve train components, keep the components in order. Follow this procedure in order to install the components in the same locations and with the same mating surfaces as when removed.

Warning: Refer to Battery Disconnect Warning in the Preface section.

Disconnect the negative battery cables before you perform any major work on the engine.