For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Wheelhouse Liner Bolt (Qty: 10) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (23 lb in)
2 | Front Bumper Fascia Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
3 | Front Bumper Fascia Retainer (Qty: 8)
4 | Front Bumper Fascia

#### Procedure

1. Unclip from front bumper fascia guides.
2. Pull forward to remove the front bumper fascia.
3. Disconnect any electrical connectors.
4. Transfer parts as needed.