For 1990-2009 cars

Callout | Component Name
--- | ---

#### Prelimary Procedure

Remove the inflatable restraint steering wheel module. Refer to Steering Wheel Inflatable Restraint Module Replacement.

1 | Steering Wheel Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 30 N·m (23 lb ft)
2 | Steering Wheel

#### Procedure

1. Disconnect electrical connectors as needed.
2. Remove the steering wheel carefully.