For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front side door trim. Refer to Front Side Door Trim Replacement.
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement.
3. Remove the outside door handle. Refer to Front Side Door Outside Handle Replacement.

1 | Front Side Door Handle Housing Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 2,5 N·m(22 lb in)
2 | Front Door Outside Handle Housing

#### Procedure

1. Disconnect the lock and handle rods to remove the housing.
2. Transfer the lock cylinder to the new housing. Refer to Front Side Door Lock Cylinder Replacement.
3. Inspect the lock, lock cylinder and handle adjustments. Refer to Front Side Door Outside Handle Rod Adjustment.