For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
3. Support the rear axle with a tall jack stand near the shock absorber.
4. Remove the upper shock absorber bolts (1).
5. Remove the lower shock absorber bolt (1).

### Installation Procedure

1. Position the shock absorber to the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install NEW upper shock absorber bolts (1) and tighten to 100 N·m (74 lb in).
3. Install NEW lower shock absorber bolt (1) and tighten to 150 N·m + 60 degrees (111 lb ft + 60 degrees).
4. Remove the jack stand.
5. Install the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
6. Lower the vehicle.