For 1990-2009 cars

Checks | Causes
--- | ---
4-5-6 Clutch Assembly |

• | Inspect for damaged, stripped or sheared splines on 4-5-6 Clutch Plates (526-528), Backing Plate (529)

• | Inspect for broken or fatiqued 4-5-6 Clutch Waved Plate (525)

• | Inspect for damaged or broken 4-5-6 Clutch Piston (520) and Piston Seals (518, 519, 521)

• | Inspect for broken or fatigued 4-5-6 Piston Return Spring (522)

• | Inspect for broken or disengaged 4-5-6 Backing Plate Retainer (532)

• | Inspect for damaged or broken 4-5-6 Clutch Dam Piston (523) and piston seals damaged, worn or delaminating

• | Inspect for broken or disengaged 4-5-6 Clutch Dam Retainer (524)

• | Inspect for stripped or sheared splines on the Reaction Carrier Hub (531)

• | Inspect for stripped or sheared splines on 3-5 Rev/4-5-6 Housing to Turbine Shaft (516)

• | Inspect for loose, worn or damaged 3-5 Rev/4-5-6 Housing Bushing

• | Inspect for broken, porous or improper surface finish or plugged oil passages of the 3-5 Rev/4-5-6 Housing (516)