For 1990-2009 cars

## Exhaust Flexible Pipe Replacement 2.0L Diesel LLW

Callout | Component Name
--- | ---
Warning: Refer to Exhaust Service Warning in the Preface section. Warning: Refer to Protective Goggles and Glove Warning in the Preface section.

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front compartment insulator. Refer to Front Compartment Insulator Replacement.

1 | Exhaust Gas Temperature Sensor Front Caution: Refer to Fastener Caution in the Preface section. Tighten 42 N·m (31 lb ft)
2 | Exhaust Flex Pipe to Catalytic Converter Nut (Qty: 3) Tighten 40 N·m (30 lb ft)
3 | Exhaust Flex Pipe to Exhaust Particulate Filter Nut (Qty: 3) Tighten 40 N·m (30 lb ft)
4 | Exhaust Pipe Front Hanger Bracket Bolt (Qty: 4) Tighten 20 N·m (15 lb ft)
5 | Exhaust Flex Pipe
6 | Exhaust Flex Pipe Gasket to Catalytic Converter
7 | Exhaust Flex Pipe Gasket to Exhaust Particulate Filter
8 | Exhaust Front Hanger Bracket Nut (Qty: 2) Tighten 20 N·m (15 lb ft)
9 | Exhaust Pipe Front Hanger Insulator (Qty: 2)

## Exhaust Flexible Pipe Replacement 1.6L LXV

Callout | Component Name
--- | ---
Warning: Refer to Exhaust Service Warning in the Preface section. Warning: Refer to Protective Goggles and Glove Warning in the Preface section.

#### Preliminary Procedure

Raise the vehicle by its full height. Refer to Lifting and Jacking the Vehicle.

1 | Exhaust Muffler Insulator (Qty: 2)
2 | Exhaust Flexible Pipe Gasket to Exhaust Rear Muffler
3 | Exhaust Pipe Front Hanger Bracket
4 | Exhaust Pipe Front Hanger Bracket Bolts and Nuts Caution: Refer to Fastener Caution in the Preface section. Tighten 20 N·m (15 lb ft)
5 | Heated Oxygen Sensor Tighten 40 N·m (30 lb ft)
6 | Catalytic Converter to Exhaust Flexible Pipe Nuts (Qty: 3) Tighten 20 N·m (15 lb ft)
7 | Catalytic Converter to Exhaust Flexible Pipe Gasket