For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove instrument panel lower trim pad cover - left side. Refer to LINK.
2. Remove instrument panel cluster trim plate. Refer to Instrument Panel Cluster Trim Plate Replacement.
3. Remove instrument panel cluster lower trim plate. Refer to LINK.
4. Remove instrument panel upper trim panel (2). Refer to Instrument Panel Upper Trim Panel Replacement.

1 | Instrument Panel Outer Air Outlet Assembly

#### Procedure

1. Remove instrument panel outer air oulet duct left side (1).
2. Remove clip (Qty: 4).