For 1990-2009 cars

#### Special Tools

• | EN 422 Installer

• | EN 45000 Remover

For equivalent regional tools, refer to Special Tools.

### Removal Procedure

1. Remove the camshaft position actuator adjuster. Refer to Camshaft Position Actuator Adjuster Replacement.
2. Remove the camshaft front oil seals (1).

### Installation Procedure

1. Insert 2 NEW camshaft front oil seals (1).
2. Install 2 sealing rings to the camshafts.
3. Tighten the seal ring with EN-422 installer (3) on the camshaft until this is in contact with the cylinder head.
4. To install, use camshaft sprocket bolt (1) in conjunction with shims (2) with a total thickness of approximately 10 mm (0.393 in).
5. Install the camshaft position actuator adjuster. Refer to Camshaft Position Actuator Adjuster Replacement.