For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
AC Compressor Bolt | 22 N·m | 17 lb ft
AC Compressor and Condenser Hose Nut | 19 N·m | 14 lb ft
AC Evaporator Hose Assembly Nut | 19 N·m | 14 lb ft
Air Intake Hose Clamps | 3.5 N·m | 31 lb in
Automatic Transmission Flex Plate Bolt | 35 N·m+30°+15° | 26 lb ft+30°+15°
Camshaft Adjuster Bolt | 65 N·m+120°+15° | 48 lb ft+120°+15°
Camshaft Adjuster Closure Plug | 30 N·m | 22 lb ft
Camshaft Bearing Cap Bolt | 8 N·m | 71 lb in
Camshaft Closure Bolt | 30 N·m | 23 lb ft
Camshaft Cover Bolt | 8 N·m | 71 lb in
Camshaft Position Actuator Solenoid Valve Bolt | 6 N·m | 54 lb in
Camshaft Position Sensor Bolt | 6 N·m | 54 lb in
Connecting Rod Bearing Cap Bolt | 35 N·m+45°+15° | 26 lb ft+45°+15°
Coolant Pipe Pump Module Bolt | 8 N·m | 71 lb in
Coolant Pipe Thermostat Housing Bolt | 8 N·m | 71 lb in
Coolant Pump Belt Pulley | 20 N·m | 15 lb ft
Coolant Pump Bolt | 8 N·m | 71 lb in
Crankshaft Balancer Bolt | 95 N·m+45°+15° | 70 lb ft+45°+15°
Crankshaft Bearing Cap Bolt | 50 N·m+45°+15° | 37 lb ft+45°+15°
Crankshaft Position Sensor Bolt | 5 N·m | 45 lb in
Cylinder Head Bolt | 25 N·m+90°+90°+90°+45° | 19 lb ft+90°+90°+90°+45°
Drive Belt Tensioner Bolt | 50 N·m | 37 lb ft
Engine Block Dampening Block Bolt Right | 50 N·m | 37 lb ft
Engine Coolant Thermostat | 8 N·m | 71 lb in
Engine Coolant Thermostat Housing | 8 N·m | 71 lb in
Engine Coolant Thermostat Housing Coolant Pipe Bolt | 8 N·m | 71 lb in
Engine Cooler Pipe Bolts | 9 N·m | 80 lb in
Engine Dampening Block Bracket Bolt Left | 55 N·m | 41 lb ft
Engine Dampening Block Bracket Bolt Right | 55 N·m | 41 lb ft
Engine Dampening Block Bracket Transmission Bolt Rear | 80 N·m | 59 lb ft
Engine Dampening Block Side Member - Left | 20 N·m | 15 lb ft
Engine Dampening Side Member Right | 35 N·m | 26 lb ft
Engine Front Cover (Oil Pump Housing) | 20 N·m | 15 lb ft
Engine Lift Front Bracket | 25 N·m | 18.5 lb ft
Engine Mount Bolt | 62 N·m | 46 lb ft
Engine Mount Bracket Bolt | 62 N·m | 46 lb ft
Engine Mount Nut | 58 N·m | 43 lb ft
Engine Oil Cooler Bolts | xx N·m | xx lb ft
Engine Oil Cooler Housing Bolt | 25 N·m | 19 lb ft
Engine Oil Cooler Inlet Pipe Bolt | 8 N·m | 71 lb in
Engine Oil Cooler Outlet Pipe Bolt | 8 N·m | 71 lb in
Engine Oil Pressure Indicator Switch | 20 N·m | 15 lb ft
Engine Oil Level Indicator Bolt | 10 N·m | 89 lb in
Evaporative Emission Canister Purge Solenoid Valve Bracket Bolt | 8 N·m | 71 lb in
Excess Pressure Valve-Bolt | 20 N·m | 15 lb ft
Exhaust Manifold Bracket Bolt | 20 N·m | 15 lb ft
Exhaust Manifold Nut | 20 N·m | 15 lb ft
Flywheel-Bolt | 35 N·m+30°+15° | 26 lb ft+30°+15°
Front Compartment Fuse Block Bolt | 22 N·m | 17 lb ft
Front Frame Bolt | 120 N·m+130° | 89 lb ft+130°
Front Engine Dampening Block Front Axle Body | 55 N·m | 40.6 lb ft
Front Engine Dampening Block Transmission | 80 N·m | 60 lb ft
Front Exhaust Pipe Bolt | 20 N·m | 15 lb ft
Generator Bolt | 35 N·m | 26 lb ft
Heated Oxygen Sensor | 40 N·m | 30 lb ft
Heat Shield Exhaust Manifold Bolt | 8 N·m | 71 lb in
Knock Sensor Bolt | 20 N·m | 15 lb ft
Ignition Module Bolt | 8 N·m | 71 lb in
Intake Manifold Absolute Pressure Sensor Bolt | 6 N·m | 54 lb in
Intake Manifold Bolt | 20 N·m | 15 lb ft
Intake Manifold Bracket to Engine Block Bolt | 8 N·m | 71 lb in
Intake Manifold Bracket Bolt | 8 N·m | 80 lb in
Multiport Fuel Injection Fuel Rail Bolt | 8 N·m | 80 lb in
Oil Filter Cap | 25 N·m | 18 lb ft
Oil Flow Check Valve Bore Plug | 21 N·m | 16 lb ft
Oil Level Indicator Tube Bolt | 8 N·m | 80 lb in
Oil Pan Bolt | 10 N·m | 89 lb in
Oil Pan Drain Plug | 14 N·m | 11 lb ft
Oil Pan Baffle Bolt | 10 N·m | 89 lb in
Oil Pan Transmission Housing Bolt M10 | 40 N·m | 30 lb ft
Oil Pan Transmission Housing Bolt M12 | 60 N·m | 45 lb ft
Oil Pressure Measurement Closure Bolt Cylinder Head | 15 N·m | 11 lb ft
Oil Pressure Switch | 20 N·m | 15 lb ft
Oil Pressure Relief Valve Closure Bolt | 21 N·m | 16 lb ft
Oil Pump Cover Bolt | 8 N·m | 71 lb in
Power Steering Fluid Reservoir Bolt | 9 N·m | 7 lb in
Rear Frame Bolt | 90 N·m+130° | 67 lb ft+130°
Rear Engine Damping Block Bracket Bolt | 55 N·m | 41 lb ft
Rear Engine Damping Block Front Axle Body Bolt | 55 N·m | 41 lb ft
Spark Plugs | 25 N·m | 19 lb ft
Throttle Body Bolt | 8 N·m | 71 lb in
Tie Rod End | 30 N·m+90°+15° | 22 lb ft+90°+15°
Timing Belt Rear Cover Bolt | 6 N·m | 54 lb in
Timing Belt Idler Pulley Bolt | 25 N·m | 19 lb ft
Timing Belt Tensioner Bolt | 20 N·m | 15 lb ft
Timing Belt Lower Front Cover Bolt | 6 N·m | 54 lb in
Timing Belt Upper Front Cover Bolt | 6 N·m | 54 lb in
Timing Belt Rear Cover Bolts | 6 N·m | 54 lb in
Torsional Vibration Damper Bolt | 95 N·m+45°+15° | 70 lb ft+45°+15°
Transmission Bolt | 75 N·m | 56 lb ft
Transmission Bracket Mount Bolt | 100 N·m | 74 lb ft
Transmission Front Mount Bolt | 58 N·m | 43 lb ft
Transmission to Cylinder Block Bolt | 60 N·m | 44 lb ft
Transmission Dampening Block Bolt Left | 35 N·m | 26 lb ft
Water Pump Pulley Bolt | 20 N·m | 15 lb ft
Wiring Harness Ground Nut | 9 N·m | 7 lb in

- (1) = Use NEW fastening nuts. (2) = Use NEW fastening bolts. (3) = Recut threads before re-use and insert bolts with screw locking compound - red. The installation time, including torque inspection, is a maximum of 10 minutes. (4) = Insert NEW fastening bolts with screw locking compound -