For 1990-2009 cars

Condition | Action
--- | ---
The battery power is low. | Confirm proper battery voltage.
The intermediate shaft dash seal is binding. | Adjust the dash seal, or replace the intermediate shaft assembly if necessary.
The intermediate shaft joints are loose or worn. | Inspect the joints and the pinch bolts for damage, and replace the intermediate shaft if necessary. Refer to Intermediate Steering Shaft Replacement.
The steering gear is binding. | If necessary, inspect and replace the steering gear. Refer to Steering Gear Replacement.
The upper steering shaft is bent. | If necessary, replace the steering column. Refer to Steering Column Replacement.
If necessary, replace the steering column. Refer to Steering Column Replacement. | Replace the steering column. Refer to Steering Column Replacement.
The sensor wire is damaged. | Replace the steering column. Refer to Steering Column Replacement.