For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the interior trim panel. Refer to Front Side Door Trim Replacement.
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement.
3. Remove the front side door lock. Refer to Front Side Door Lock Replacement.

1 | Front Side Door Lock Rod

#### Procedure

Inspect the lock, lock cylinder and handle adjustments. Refer to Front Side Door Outside Handle Rod Adjustment.