For 1990-2009 cars

### Removal Procedure

1. Remove instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement.
2. Remove instrument panel wiring harness (2) from instrument panel tie bar (1).

Disconnect electrical connectors.

3. Remove instrument panel tie bar (2).

• | Remove 4 instrument panel tie bar bolts (3, 4).

• | Remove 2 instrument panel tie bar nuts (1).

4. Remove mode control cam (1).

### Installation Procedure

Note: The mode control cam can only be fitted in one position.

1. Install mode control cam (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install instrument panel tie bar (2).

• | Install 4 instrument panel tie bar bolts (3, 4) and tighten to XXX N·m(XXX lb in) .

• | Install 2 instrument panel tie bar nuts (1) and tighten to XXX N·m(XXX lb in) .

3. Install instrument panel wiring harness (2) from instrument panel tie bar (1).

Connect electrical connectors.

4. Install instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement.