For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Glass and Sheet Metal Handling Warning in the Preface section.

#### Preliminary Procedure

1. Remove the front side door trim. Refer to Front Side Door Trim Replacement.
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement.

1 | Front Side Door Window Regulator Sash Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Side Door Window

#### Procedure

1. Loosen the window regulator sash nuts.
2. Connect the door trim panel wire connector.

Note: Start the vehicle to ensure maximum power to the window motor. This is required in order to fully seat the window for adjustment.

3. Start the vehicle.
4. Using the power window switch, raise the window to the full up position.
5. Tighten the front side door window regulator sash nuts.
6. Inspect for proper window operation and a tight seal.
7. Shut off the vehicle.