For 1990-2009 cars

#### Special Tools

EN-6333 Locking Pin

For equivalent regional tools, refer to Special Tools.

Note: Observe direction of rotation.

1. Insert the timing belt (1).
2. Apply tension to the timing belt tensioner (2) in the direction of the arrow, using an Allen key (1).
3. Remove the EN 6333 locking pin (3).

Note: The timing belt tensioner moves automatically to the correct position.

4. Release tension on timing belt tensioner.