For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the steering column upper trim cover. Refer to Steering Column Upper Trim Cover Replacement.
2. Remove the steering column lower trim cover. Refer to Steering Column Lower Trim Cover Replacement.

1 | Turn Signal Switch

#### Procedure

1. Disconnect any electrical connectors as needed.
2. Release the plastic retaining tabs to release the turn signal switch from steering wheel inflatable restraint module coil.