For 1990-2009 cars

Note: Coat the gasket with new engine oil.

1. Install a NEW engine oil cooler gasket (6).

Note: Consider the marked installation position.

2. Install the engine oil cooler (7).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the engine oil cooler bolt (8) and tighten to 40 N·m (30 lb ft).

Note: Coat the gasket with new engine oil.

4. Install a NEW oil filter housing gasket (9).
5. Install the oil filter housing (10).
6. Install the oil filter housing bolt (11) and tighten to 50 N·m (37 lb ft).
7. Install the oil filter housing oil drain plug gasket (5)
8. Install the oil filter housing oil drain plug (4) and tighten to XXX N·m (XXX lb ft).
9. Install a NEW oil filter (3).
10. Install the oil filter cap (1) with a NEW oil filter cap gasket (2) and tighten to 25 N·m (19 lb ft).